6. Control Codes STAR mode
*6-1. Control Codes Used in Character Setting
 <ESC> "R" n 1B 52 n Select international character set. 
      Default is according to the dip switch settings 3, 4 and 5.
 <ESC> "M" 1B 4D Select 7 ´ 7 (Half dots) character size (Default setting)
 <ESC> "P" 1B 50 Select 9 ´ 7 (Half dots) character size
 <SO> 0E Select expanded character mode
 <SI> 0F Cancel expanded character mode (Default setting)
 <DC4> 14 Cancel expanded character mode (Default setting)
 <ESC> "W" "1" 1B 57 31 Select expanded character mode
 <ESC> "W" <1> 1B 57 01
 <ESC> "W" "0" 1B 57 30 Cancel expanded character mode
 <ESC> "W" <0> 1B 57 00 (Default setting)
*6-2. Control Codes Used in Print Mode Setting
 <ESC> "4" 1B 34 Red color print selection (enable for SP216)
 <ESC> "5" 1B 35 Red color print deselection (enable for SP216) (Default setting)
 <ESC> "E" 1B 45 Emphasized print mode selection
 <ESC> "F" 1B 46 Emphasized print mode deselection (Default setting)
*6-3. Control Codes Used in Line Spacing
 <LF> 0A Line feed
 <CR> 0D Line feed (same as LF)
 <ESC> "a" n 1B 61 n Feed paper n lines
*6-4. Control Codes Used for Peripheral Units
 <ESC> <BEL> n1 n2 1B 07 n1 n2 Adjust drive pulse width for peripheral unit (Default setting)
 <BEL> 07 Deferred drive command "A" for peripheral unit 1
 <FS> 1C Immediate drive command "B" for peripheral unit 1
*6-5. Auto Cutter Control (SP240 type only)
 <ESC> "d" "0" 1B 64 30 Full-cut command to the auto cutter
 <ESC> "d" <0> 1B 64 00
 <ESC> "d" "1" 1B 64 31 Partial-cut command to the auto cutter
 <ESC> "d" <1> 1B 64 01
*6-6. Other Control Codes
 <CAN> 18 Cancel print data in buffer
 <ESC> "@" 1B 40 Initialize printer
 <ESC> "e" "0" 1B 65 30 ON LINE/FEED switch valid
 <ESC> "e" <0> 1B 65 00 (Default setting)
 <ESC> "e" "1" 1B 65 31 ON LINE/FEED switch invalid
 <ESC> "e" <1> 1B 65 01
 <ESC> "f" "0" 1B 66 30 ON LINE switch valid
 <ESC> "f" <0> 1B 66 00 (Default setting)
 <ESC> "f" "1" 1B 66 31 ON LINE switch invalid
 <ESC> "f" <1> 1B 66 01
